Frame a Wall Checklist Checklist:

materials:

* Sketch pad
* Masking tape
* Needle nose pliers
* Palette or Putty knife
* Making Tape
* Tape measure
* Carpet knife or Utility knife
* Tin snips/ metal cutters
* 2” x 4” wood lumber (various lengths)
* Metal channel (3 5/8” wide), available in 10’ lengths
* 1 ¼” Drywall screws
* 2 ½” screws
* 3” screws
* Carpenter’s Square
* Marker or pencil
* Powder actuated nailer & bullet BLANKS
* Hammer
* Level
* Miter saw
* Drill & bits (for drilling and driving screws)
* Safety glasses
* Sliding bevel (if necessary)
* Utility gloves
* Wood (cedar) shims
* 2 ½” finish nails
* Construction glue (low VOC) & Caulk gun

**Welcome to your newly designed space! -Renee**